1. Flash SD card with Isaac-Ros Image and insert into the Jetson. Power on the device no
2. Setting up SPI

* In opt/nvidia/jetson-io:
* Call sudo python3 jetson-io.py
  + Select options to activate spi1 and I2S
* Verify by calling sudo python3 io-config-by-pins.py
* Call sudo modprobe spidev

1. If you have issues with dev/ttyUSB0, you may need to call sudo apt remove brltty
2. Connect the corresponding SPI pins on the header to the SPI pins on the MCU control board